## Uses of Class
javax.print.attribute.standard.PrinterStateReason

- Packages that use PrinterStateReason
  Package | Description
  --- | ---
  javax.print.attribute.standard | Package `javax.print.attribute.standard` contains classes for specific printing attributes.

- - ### Uses of PrinterStateReason in javax.print.attribute.standard

    Fields in javax.print.attribute.standard declared as PrinterStateReason
    Modifier and Type | Field | Description
    --- | --- | ---
    `static PrinterStateReason` | PrinterStateReason.`CONNECTING_TO_DEVICE` | The printer has scheduled a job on the output device and is in the process of connecting to a shared network output device (and might not be able to actually start printing the job for an arbitrarily long time depending on the usage of the output device by other servers on the network).
    `static PrinterStateReason` | PrinterStateReason.`COVER_OPEN` | One or more covers on the device are open.
    `static PrinterStateReason` | PrinterStateReason.`DEVELOPER_EMPTY` | The device is out of developer.
    `static PrinterStateReason` | PrinterStateReason.`DEVELOPER_LOW` | The device is low on developer.
    `static PrinterStateReason` | PrinterStateReason.`DOOR_OPEN` | One or more doors on the device are open.
    `static PrinterStateReason` | PrinterStateReason.`FUSER_OVER_TEMP` | The fuser temperature is above normal.
    `static PrinterStateReason` | PrinterStateReason.`FUSER_UNDER_TEMP` | The fuser temperature is below normal.
    `static PrinterStateReason` | PrinterStateReason.`INPUT_TRAY_MISSING` | One or more input trays are not in the device.
    `static PrinterStateReason` | PrinterStateReason.`INTERLOCK_OPEN` | One or more interlock devices on the printer are unlocked.
    `static PrinterStateReason` | PrinterStateReason.`INTERPRETER_RESOURCE_UNAVAILABLE` | An interpreter resource is unavailable (e.g., font, form).
    `static PrinterStateReason` | PrinterStateReason.`MARKER_SUPPLY_EMPTY` | The device is out of at least one marker supply (e.g. toner, ink, ribbon).
    `static PrinterStateReason` | PrinterStateReason.`MARKER_SUPPLY_LOW` | The device is low on at least one marker supply (e.g. toner, ink, ribbon).
    `static PrinterStateReason` | PrinterStateReason.`MARKER_WASTE_ALMOST_FULL` | The device marker supply waste receptacle is almost full.
    `static PrinterStateReason` | PrinterStateReason.`MARKER_WASTE_FULL` | The device marker supply waste receptacle is full.
    `static PrinterStateReason` | PrinterStateReason.`MEDIA_EMPTY` | At least one input tray is empty.
    `static PrinterStateReason` | PrinterStateReason.`MEDIA_JAM` | The device has a media jam.
    `static PrinterStateReason` | PrinterStateReason.`MEDIA_LOW` | At least one input tray is low on media.
    `static PrinterStateReason` | PrinterStateReason.`MEDIA_NEEDED` | A tray has run out of media.
    `static PrinterStateReason` | PrinterStateReason.`MOVING_TO_PAUSED` | Someone has paused the printer, but the device(s) are taking an appreciable time to stop.
    `static PrinterStateReason` | PrinterStateReason.`OPC_LIFE_OVER` | The optical photo conductor is no longer functioning.
    `static PrinterStateReason` | PrinterStateReason.`OPC_NEAR_EOL` | The optical photo conductor is near end of life.
    `static PrinterStateReason` | PrinterStateReason.`OTHER` | The printer has detected an error other than ones listed below.
    `static PrinterStateReason` | PrinterStateReason.`OUTPUT_AREA_ALMOST_FULL` | One or more output areas are almost full (e.g. tray, stacker, collator).
    `static PrinterStateReason` | PrinterStateReason.`OUTPUT_AREA_FULL` | One or more output areas are full (e.g. tray, stacker, collator).
    `static PrinterStateReason` | PrinterStateReason.`OUTPUT_TRAY_MISSING` | One or more output trays are not in the device.
    `static PrinterStateReason` | PrinterStateReason.`PAUSED` | Someone has paused the printer and the printer's `PrinterState` is `STOPPED`.
    `static PrinterStateReason` | PrinterStateReason.`SHUTDOWN` | Someone has removed a printer from service, and the device may be powered down or physically removed.
    `static PrinterStateReason` | PrinterStateReason.`SPOOL_AREA_FULL` | The limit of persistent storage allocated for spooling has been reached.
    `static PrinterStateReason` | PrinterStateReason.`STOPPED_PARTLY` | When a printer controls more than one output device, this reason indicates that one or more output devices are stopped.
    `static PrinterStateReason` | PrinterStateReason.`STOPPING` | The printer is in the process of stopping the device and will be stopped in a while.
    `static PrinterStateReason` | PrinterStateReason.`TIMED_OUT` | The server was able to connect to the output device (or is always connected), but was unable to get a response from the output device.
    `static PrinterStateReason` | PrinterStateReason.`TONER_EMPTY` | The device is out of toner.
    `static PrinterStateReason` | PrinterStateReason.`TONER_LOW` | The device is low on toner.

    Methods in javax.print.attribute.standard that return types with arguments of type PrinterStateReason
    Modifier and Type | Method | Description
    --- | --- | ---
    `Set<PrinterStateReason>` | PrinterStateReasons.`printerStateReasonSet​(Severity severity)` | Obtain an unmodifiable set view of the individual printer state reason attributes at the given severity level in this `PrinterStateReasons` attribute.

    Methods in javax.print.attribute.standard with parameters of type PrinterStateReason
    Modifier and Type | Method | Description
    --- | --- | ---
    `Severity` | PrinterStateReasons.`put​(PrinterStateReason reason, Severity severity)` | Adds the given printer state reason to this printer state reasons attribute, associating it with the given severity level.

    Constructor parameters in javax.print.attribute.standard with type arguments of type PrinterStateReason
    Constructor | Description
    --- | ---
    `PrinterStateReasons​(Map<PrinterStateReason,​Severity> map)` | Construct a new printer state reasons attribute that contains the same `PrinterStateReason`-to-`Severity` mappings as the given map.