Module java.management
Package javax.management.monitor

## Interface GaugeMonitorMBean

- All Superinterfaces:
    `MonitorMBean`
  All Known Implementing Classes:
    `GaugeMonitor`

      public interface GaugeMonitorMBean
      extends MonitorMBean

  Exposes the remote management interface of the gauge monitor MBean.
  Since:
    1.5

- - ### Method Summary

    Modifier and Type | Method | Description
    --- | --- | ---
    `Number` | `getDerivedGauge()` | Deprecated. As of JMX 1.2, replaced by `getDerivedGauge(ObjectName)`
    `Number` | `getDerivedGauge​(ObjectName object)` | Gets the derived gauge for the specified MBean.
    `long` | `getDerivedGaugeTimeStamp()` | Deprecated. As of JMX 1.2, replaced by `getDerivedGaugeTimeStamp(ObjectName)`
    `long` | `getDerivedGaugeTimeStamp​(ObjectName object)` | Gets the derived gauge timestamp for the specified MBean.
    `boolean` | `getDifferenceMode()` | Gets the difference mode flag value.
    `Number` | `getHighThreshold()` | Gets the high threshold value.
    `Number` | `getLowThreshold()` | Gets the low threshold value.
    `boolean` | `getNotifyHigh()` | Gets the high notification's on/off switch value.
    `boolean` | `getNotifyLow()` | Gets the low notification's on/off switch value.
    `void` | `setDifferenceMode​(boolean value)` | Sets the difference mode flag value.
    `void` | `setNotifyHigh​(boolean value)` | Sets the high notification's on/off switch value.
    `void` | `setNotifyLow​(boolean value)` | Sets the low notification's on/off switch value.
    `void` | `setThresholds​(Number highValue, Number lowValue)` | Sets the high and the low threshold values.

    - ### Methods declared in interface javax.management.monitor.MonitorMBean

      `addObservedObject, containsObservedObject, getGranularityPeriod, getObservedAttribute, getObservedObject, getObservedObjects, isActive, removeObservedObject, setGranularityPeriod, setObservedAttribute, setObservedObject, start, stop`

- - ### Method Detail

    - #### getDerivedGauge

          @Deprecated
          Number getDerivedGauge()

      Deprecated.
      As of JMX 1.2, replaced by `getDerivedGauge(ObjectName)`
      Gets the derived gauge.
      Returns:
        The derived gauge.

    - #### getDerivedGaugeTimeStamp

          @Deprecated
          long getDerivedGaugeTimeStamp()

      Deprecated.
      As of JMX 1.2, replaced by `getDerivedGaugeTimeStamp(ObjectName)`
      Gets the derived gauge timestamp.
      Returns:
        The derived gauge timestamp.

    - #### getDerivedGauge

          Number getDerivedGauge​(ObjectName object)

      Gets the derived gauge for the specified MBean.
      Parameters:
        `object` - the MBean for which the derived gauge is to be returned
      Returns:
        The derived gauge for the specified MBean if this MBean is in the set of observed MBeans, or `null` otherwise.

    - #### getDerivedGaugeTimeStamp

          long getDerivedGaugeTimeStamp​(ObjectName object)

      Gets the derived gauge timestamp for the specified MBean.
      Parameters:
        `object` - the MBean for which the derived gauge timestamp is to be returned
      Returns:
        The derived gauge timestamp for the specified MBean if this MBean is in the set of observed MBeans, or `null` otherwise.

    - #### getHighThreshold

          Number getHighThreshold()

      Gets the high threshold value.
      Returns:
        The high threshold value.

    - #### getLowThreshold

          Number getLowThreshold()

      Gets the low threshold value.
      Returns:
        The low threshold value.

    - #### setThresholds

          void setThresholds​(Number highValue,
                             Number lowValue)
                      throws IllegalArgumentException

      Sets the high and the low threshold values.
      Parameters:
        `highValue` - The high threshold value.
        `lowValue` - The low threshold value.
      Throws:
        `IllegalArgumentException` - The specified high/low threshold is null or the low threshold is greater than the high threshold or the high threshold and the low threshold are not of the same type.

    - #### getNotifyHigh

          boolean getNotifyHigh()

      Gets the high notification's on/off switch value.
      Returns:
        `true` if the gauge monitor notifies when exceeding the high threshold, `false` otherwise.
      See Also:
        `setNotifyHigh(boolean)`

    - #### setNotifyHigh

          void setNotifyHigh​(boolean value)

      Sets the high notification's on/off switch value.
      Parameters:
        `value` - The high notification's on/off switch value.
      See Also:
        `getNotifyHigh()`

    - #### getNotifyLow

          boolean getNotifyLow()

      Gets the low notification's on/off switch value.
      Returns:
        `true` if the gauge monitor notifies when exceeding the low threshold, `false` otherwise.
      See Also:
        `setNotifyLow(boolean)`

    - #### setNotifyLow

          void setNotifyLow​(boolean value)

      Sets the low notification's on/off switch value.
      Parameters:
        `value` - The low notification's on/off switch value.
      See Also:
        `getNotifyLow()`

    - #### getDifferenceMode

          boolean getDifferenceMode()

      Gets the difference mode flag value.
      Returns:
        `true` if the difference mode is used, `false` otherwise.
      See Also:
        `setDifferenceMode(boolean)`

    - #### setDifferenceMode

          void setDifferenceMode​(boolean value)

      Sets the difference mode flag value.
      Parameters:
        `value` - The difference mode flag value.
      See Also:
        `getDifferenceMode()`